cntrl_fifo |

2019.03.29.13:34:05 | Datasheet

Overview

Memory Map

## fifo_0

fifo v18.1

## Parameters
DEVICE_FAMILY | ARRIA10
GUI_Clock | 4
GUI_CLOCKS_ARE_SYNCHRONIZED | 0
GUI_delaypipe | 5
GUI_synStage | 3
GUI_LegacyRREQ | 1
GUI_RAM_BLOCK_TYPE | Auto
GUI_Optimize | 0
GUI_Optimize_max | 0
GUI_Width | 1
GUI_Depth | 256
GUI_output_width | 8
GUI_AlmostFullThr | 1
GUI_AlmostEmptyThr | 1
GUI_MAX_DEPTH | Auto
GUI_DISABLE_DCFIFO_EMBEDDED_TIMING_CONSTRAINT | true
GUI_diff_widths | false
GUI_Full | true
GUI_Empty | true
GUI_UsedW | true
GUI_AlmostFull | false
GUI_AlmostEmpty | false
GUI_sc_aclr | false
GUI_sc_sclr | false
GUI_rsFull | false
GUI_rsEmpty | true
GUI_rsUsedW | false
GUI_wsFull | true
GUI_wsEmpty | false
GUI_wsUsedW | false
GUI_msb_usedw | false
GUI_dc_aclr | false
GUI_write_aclr_synch | false
GUI_read_aclr_synch | false
GUI_OVERFLOW_CHECKING | false
GUI_UNDERFLOW_CHECKING | false
GUI_LE_BasedFIFO | false
GUI_MAX_DEPTH_BY_9 | false
GUI_ENABLE_ECC | false
GUI_Usedw_width | 8
GUI_RdUsedw_width | 8
GUI_WrUsedw_width | 8
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

generation took 0.00 seconds | rendering took 0.00 seconds