LpGBT_DP |

2020.06.02.16:25:46 | Datasheet

Overview

Memory Map

## ram_2port_0

ram_2port v18.1

## Parameters
DEVICE_FAMILY | ARRIA10
GUI_MODE | 0
GUI_MEM_IN_BITS | 0
GUI_MEMSIZE_BITS | 256
GUI_MEMSIZE_WORDS | 4096
GUI_QA_WIDTH | 36
GUI_QB_WIDTH | 36
GUI_DATAA_WIDTH | 36
GUI_MAX_DEPTH | Auto
GUI_WIDTH_ECCENCPARITY | 8
GUI_TBENCH | false
GUI_VAR_WIDTH | false
GUI_RAM_BLOCK_TYPE | Auto
GUI_LC_IMPLEMENTION_OPTIONS | 0
GUI_FILE_REFERENCE | 0
GUI_CLOCK_TYPE | 1
GUI_RDEN_SINGLE | false
GUI_RDEN_DOUBLE | false
GUI_BYTE_ENABLE_A | false
GUI_BYTE_ENABLE_B | false
GUI_ECC_DOUBLE | false
GUI_ECC_TRIPLE | false
GUI_ECC_PIPELINE | false
GUI_ECCENCBYPASS | false
GUI_COHERENT_READ | false
GUI_FORCE_TO_ZERO | false
GUI_BYTE_ENABLE_WIDTH | 8
GUI_WRITE_INPUT_PORTS | true
GUI_READ_INPUT_RDADDRESS | true
GUI_READ_OUTPUT_QA | true
GUI_READ_OUTPUT_QB | true
GUI_DIFFERENT_CLKENS | false
GUI_CLKEN_WRITE_INPUT_REG | false
GUI_CLKEN_READ_INPUT_REG | false
GUI_CLKEN_READ_OUTPUT_REG | false
GUI_CLKEN_INPUT_REG_A | false
GUI_CLKEN_INPUT_REG_B | false
GUI_CLKEN_OUTPUT_REG_A | false
GUI_CLKEN_OUTPUT_REG_B | false
GUI_CLKEN_ADDRESS_STALL_A | false
GUI_CLKEN_ADDRESS_STALL_B | false
GUI_CLKEN_WRADDRESSSTALL | false
GUI_CLKEN_RDADDRESSSTALL | false
GUI_ACLR_READ_INPUT_RDADDRESS | false
GUI_ACLR_READ_OUTPUT_QA | false
GUI_ACLR_READ_OUTPUT_QB | false
GUI_SCLR_READ_OUTPUT_QA | false
GUI_SCLR_READ_OUTPUT_QB | false
GUI_Q_PORT_MODE | 2
GUI_CONSTRAINED_DONT_CARE | true
GUI_RDW_A_MODE | New Data
GUI_RDW_B_MODE | New Data
GUI_NBE_A | true
GUI_NBE_B | true
GUI_BLANK_MEMORY | 0
GUI_INIT_FILE_LAYOUT | PORT_B
GUI_INIT_SIM_TO_X | false
GUI_MIF_FILENAME |
GUI_BYTE_WIDTH | 0
GUI_MODULE_NAME | altera_syncram
GUI_DATA_WIDTH | 36
GUI_Q_WIDTH | 36
GUI_WRADDRESS_WIDTH | 12
GUI_RDADDRESS_WIDTH | 12
GUI_WIDTH_ECCSTATUS | 2
GUI_NUMWORDS_A | 4096
GUI_NUMWORDS_B | 4096
GUI_RESOURCE_USAGE | 8 M20K
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

generation took 0.00 seconds | rendering took 0.01 seconds