alt_sld_fab |

2020.06.25.16:01:45 | Datasheet

Overview

Memory Map

## alt_sld_fab

alt_sld_fab v18.1

## Parameters
DESIGN_HASH | b660d55950f9852630e8
NODE_COUNT | 2
MAX_WIDTH | 2
SETTINGS | {fabric a10_xcvr dir agent use_clock 0 needs_clock 0 psig 6b6bab39} {fabric a10_xcvr dir agent use_clock 0 needs_clock 0 psig 6b6bab39}
CLOCKS | {id {} } {id {} }
AGENTS |
EP_INFOS | {hpath {lpgbtFpga_top:f0|Altera_10G_TX:mgt_inst|TX_10G:t0|TX_10G_altera_xcvr_native_a10_181_cylqohi:xcvr_native_a10_0|altera_transceiver_reset_endpoint:g_xcvr_native_insts[0].g_analog_resets_default.g_tre_tx_endpoint.reset_endpoint_tx|altera_a10_xcvr_reset_endpoint:xcvr_reset_ep_inst|altera_fabric_endpoint:ep} } {hpath {lpgbtFpga_top:f0|Altera_10G_TX:mgt_inst|TX_10G:t0|TX_10G_altera_xcvr_native_a10_181_cylqohi:xcvr_native_a10_0|altera_transceiver_reset_endpoint:g_xcvr_native_insts[0].g_analog_resets_default.g_tre_rx_endpoint.reset_endpoint_rx|altera_a10_xcvr_reset_endpoint:xcvr_reset_ep_inst|altera_fabric_endpoint:ep} }
MIRROR | 0
TOP_HUB | 1
COMPOSED_SETTINGS | {fabric a10_xcvr dir agent use_clock 0 needs_clock 0} {fabric a10_xcvr dir agent use_clock 0 needs_clock 0}
DEVICE_FAMILY | ARRIA10
AUTO_DEVICE | Unknown
AUTO_DEVICE_SPEEDGRADE | Unknown
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## alt_sld_fab_presplit

altera_super_splitter v18.1

## Parameters
MAX_WIDTH | 2
SEND_WIDTHS | 2 2
RECEIVE_WIDTHS | 1 1
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## alt_sld_fab_splitter

altera_sld_splitter v18.1

alt_sld_fab_presplit | pass | alt_sld_fab_splitter
nodes
|  | reset_0 | alt_sld_fab_a10xcvrfabric
|  | reset_0
|  | reset_1
|  | reset_1

## Parameters
FRAGMENTS | {{name reset type conduit dir start ports { {tre_reset_req tre_reset_req out 1 0} {tre_reset_in tre_reset_in in 1 0} {clk_in clk_in out 1 1} } } } {{name reset type conduit dir start ports { {tre_reset_req tre_reset_req out 1 0} {tre_reset_in tre_reset_in in 1 0} {clk_in clk_in out 1 1} } } }
EXAMPLE |
ADD_INTERFACE_ASGN | 0
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

## alt_sld_fab_a10xcvrfabric

altera_a10_xcvr_reset_sequencer v18.1

alt_sld_fab_splitter | reset_0 | alt_sld_fab_a10xcvrfabric
reset_0
reset_1
reset_1

## Parameters
SETTINGS | {use_clock 0 needs_clock 0} {use_clock 0 needs_clock 0}
COUNT | 2
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

generation took 0.01 seconds | rendering took 0.03 seconds